DAWN DANCER
60FT NARROWBOAT — SALES PARTICULARS

Vessel Identification & Exterior
	Vessel Name
	Dawn Dancer

	Registration No.
	517264 (Index No. 108)

	Length
	60ft (18.28m)

	Region
	Kennet & Avon

	Coachwork & Livery
	Deep navy blue primary panels with cream upper borders, deep red lower hull bands, and traditional white signwriting. Porthole windows fitted with polished brass bezels.
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	Stern & Deck
	[image: ]Traditional aft deck layout features a highly decorated barber-pole tiller pin. Aft doors display exquisite hand-painted traditional 'Roses and Castles' detailing.




Engineering & Electrical Architecture
	Power Management
	Victron Energy Digital Multi Control (Inverter/Charger) paired with a Victron Energy BMV-700 Battery Monitor, ensuring precise oversight of the vessel's power state.
[image: ]

	Electrical Distribution
	L&T Marine bespoke distribution panel offering isolated 12V DC (Pumps, Navigation, Aux) and 230V AC (Sockets, Mains) circuits. Professional marine-grade switching and breakers.

	
Domestic Battery Bank
	
Heavy-duty red domestic storage cells, safely secured with webbing straps within a purpose-built structural timber enclosure. Professional high-gauge cabling and crimped terminal isolation.

	Heating Systems
	Webasto diesel-fired central heating system (control interface adjacent to the main electrical board), supplemented by a solid fuel multi-stove located in the forward saloon. Panel radiators installed throughout.



Interior Layout & Accommodation
	Saloon
	Open-plan forward saloon trimmed in light ash/oak veneered panelling. Furnished with twin cream leather swivel recliner chairs and footstools. Port-side solid fuel stove, corner entertainment cabinetry, and a space-saving drop-leaf dining table stowed beneath the starboard gunwale.
[image: ]

	Galley
	Generous U-shaped aft galley featuring dark stone-effect laminate work surfaces and complementary tiled splashbacks. Domestic-sized four-burner gas hob with separate oven and grill. Under-counter 12V/230V refrigerator. Integrated Panasonic microwave oven positioned on custom shelving. Stainless steel circular sink with monobloc mixer tap and dedicated drinking water filter tap.
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Cruising Inventory & Ancillaries
The vessel is fully equipped for immediate active cruising. A dedicated utility locker houses essential deck hardware in an organised manner, including:
Heavy-duty mooring chains and nappy pins for varied piling and towpath moorings.
Multiple lock windlasses and a traditional wooden mooring mallet.
Deck umbrella and general boatman's operational equipment.

Strictly factual brokerage details compiled for reference. Measurements and specifications are provided for guidance and should be verified independently.
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